**M210(S5PV210)How To Porting Telnet**

[**http://www.mangoboard.com/**](http://www.mangoboard.com/)

**Microsoft Corporation**

**Registered User**

**Document History**

|  |  |  |
| --- | --- | --- |
| **Revision** | **Date** | **Change note** |
|  |  |  |
|  |  |  |

목차

[1. How To Configure BuildRoot(Busybox) 4](#_Toc355267334)

[2. How To Test Telnet 4](#_Toc355267335)

# **How To Configure BuildRoot(Busybox)**

|  |
| --- |
| $ cd output/build/busybox-1.20.1/ |
| $ make menuconfig |
| Networking Utilities ---> |
| [\*] inetd x x  x x [\*] Support echo service (NEW) x x  x x [\*] Support discard service (NEW) x x  x x [\*] Support time service (NEW) x x  x x [\*] Support daytime service (NEW) x x  x x [\*] Support chargen service (NEW) x x  x x [\*] Support RPC services (NEW) |
| x x [\*] telnet x x  x x [\*] Pass TERM type to remote host x x  x x [\*] Pass USER type to remote host x x  x x [\*] telnetd x x  x x [\*] Support standalone telnetd (not inetd only) (NEW) x x  x x [\*] Support -w SEC option (inetd wait mode) (NEW) |
| [\*] tcpsvd |

|  |
| --- |
| $rm -f .stamp\_built .stamp\_configured .stamp\_target\_installed |
| $ cp .config ../../../package/busybox/busybox-1.20.x.config |

|  |
| --- |
| $ cd - |
| $ ./build\_rootfs.sh |

# **How To Test Telnet**

보드 부팅 하고, 랜선 연결후,

|  |
| --- |
| #ifconfig eth0 192.168.10.100 |
| #inetd |

Host PC에서

|  |
| --- |
| $ telnet 192.168.10.100 |
| Trying 192.168.10.100...  Connected to 192.168.10.100.  Escape character is '^]'. |
| mango210 login: **default** |
| $ ls  $ pwd  /home/default |

테스트로 default란 id를 가지고, 로그인을 했습니다.

다른 ID를 사용하시려면, useradd를 이용하여, 추가하신 이후에, 하시면 될 것 같습니다.